CLUB	kHz	UTC	DD	MM	ITU	IDENT	MODE	 BD                                          	SH	DETAILS	
NZART	3560	0900-2100	DY	05	3	 B.C. Stn	A3E	--	--	R. Pyongyang B.C. Stn.	
   "	3880
3890	1700-	DY	05	3	unide	A3Exxx	 --	 --	Shifts between these 2 frequencies. unid B.C. and Jammers.	
   "	7000-7020	0935-	29	05	3	Unid	PXX	 --	 --	O.T.H.R. Chinese, centred on 6980kHz.	
   "	   "  	1845-	30	05	3	Unid	PXX	 --	 --	    "             "             "	
   "	7000	HX24	DY	05	3	Unid	J3E/U/L	 -- 	 --	Indonesian C.Bers.	
   "	7039	H24	DY	05	3	Unid	A1A	  --	 --	Beacons M,D,C,S,F and K.	
   "	7054	1700-1900	DY	05	3	REA4	F1B	 --	 --	Moscoe maritime.	
   "	7089.5	1815-2105	02-17	05	3	Unid	A3E	 --	 --	 B.C. Stn, unidentified.	
   "	7090	1110	10	05	3	Unid	A1E	 --	 --	Steady carrier, see attached note.	
   "	7092	1830-	29	05	3	Unid	F7D	 --	 250Hz	8x250 Hz channels.	
   "	   "	1845-	30	05	3	Unid	F7D	 --	 250Hz	8x259 Hz channels.	
   "	7100	1700-1900	DY	05	3	Unid	A3E	 --	 --	Unidentified B.C. stn.	
   "	14000	HX24	DY	05	3	Unid	J3E/U/L	 --	 --	Indonesian C.Bers	
   "	14002	0930-	29	05	3	Unid	F7B	 --	 --	4f data burst, Chinese	
   "	14008	HX0830-0930	DY	05	3	Unid	F1B	 --	 250Hz	Russian Navy.	
   "	14026	1945-	05	05	3	Unid	M7B	 --	 --	Multi-channel, phase modulated	
   "	14052	0925-	29	05	3	Unid	F7D	 --	250Hz`	8x250Hz channels	
   "	14100	213--2300	13	05	3	Unid	A3E	 --	 --	Unidentified B,C, Stn.	
   "	14100	HX24	DY	05	3	Unid	J3E/U/L	 --	 --	Indonesian C.Bers.	
   "	14104	0830-	18	05	3	Unid	F1B	 --	250Hz	Encripted	
   "	14104	0745-0830	23	05	3	Unid	F1B	 --	250Hz	Encripted.	
   "	14105	HX24	DY	05	3	Unid	J3E/U	 --	 --	Indonesian C.Bers.	
   "	14120	0745-	23	05	3	Unid	F1B	 --	250Hz	Encripted.	
   "	14120	0645	25	05	3	Unid	F1B	 --	250Hz	Encripted.	
   "	14122	0830-	18	05	3	Unid	M7B	 --	 --	Multi-channel, phase modulated.	
   "	14192	1745-2000	03	05	3	Unid	F1B	 --	 --	Idle signals only	
   "	14250	0400-0900	DY	05	3	B.C. Stn.	A3E	 --	 --	Radio Pyongyang.	
   "	14280	0800-0930	DY	05	3	B.C. Stn	A3E	 --	 --	 2f of B.C. on 7140 kHz.	
   "	24950+/-25	H24	DY	05	3	Unid	PXX	 --	 --	'Codar' sea state radar.	
   "	28000+++	H24	DY	05	3	Unid	A3E	 --	 --	Chinese C.B. every 5 kHz.	
											
NOTE.	7090	1110	10	05	3	Unid	A1E			Steady carrier, no modulation. S5x5	
         	   "	1146	11	05	3	Unid	A1E			S5X9+10	
	   "	1133	12	05	3	Unid	A1E			S5X6.	
	   "	1230	13	05	3	Unid	A1E			S5X7.	
	   "	1046	14	05	3	Unid	A1E			S5X3 to 6	
	   "	0756	15	05	3	Unid	A1E			S5X1to2, very weak.	
	   "	1048	16	05	3	Unid	A1E			S5X3, very weak.	
	   "	0720	17	05	3	Unid	A1E			S5X2, very weak.	
	   "	1105	18	05	3	Unid	A1E			S5X3 to 5.	
	   "	1140	19	05	3	Unid	A1E			S5X5.	
	   "	0808	20	05	3	Unid	A1E			S5X3.	
	   "	1132	21	05	3	Unid	A1E			S5X5.	
	   "	1000-	22	05	3	Unid	A1E			S5X9+10	
	   "	1042-	23	05	3	Unid	A1E			S5X5	
	   "	1938-	23	05	3	Unid	A1E			Fading into the noise level.	
	   "	1036	24	05	3	Unid	A1E			S5X9	
	   "	1230	24	05	3	Unid	A1E			S5X9.Starting to test.	
	   "	1146	"	"	"	"	"			Sewries of dota and dashes NOT Cw.	
		1147	"	'	'	"	"			2 series of 2 dots followed by a long dash.	
	  "	1150	"	"	"	"	"			K, T, in morse followed by a series of dots, voices in background then off the air.  Two bearing were obtained, one from Auckland and one from just north of wellington, bothe indicated NE of New Zealand.  Inquiries with Radio New Zealand and M.E.D. (Our Licensing Authority) showed that no New Zealand stations were using that frequency or were testing.  I have not heard it since the 24-5-06.	
ARSI	7005	0230	22	05	3	CLN	J3EU			Fishing trawlers of Sri Lanka	
ARSI	7006	0140	26	05	3	CLN	J3EU			Fishing trawlers of Sri Lanka	
ARSI	7045	0300	DY	05	3	IND	A3E			AIR Chennai spurious,2Audios.	
ARSI	7053	0230	DY	05	3	IND	N0N			AIR-TVM,5 spur N0N freqs.	
ARSI	7073	0142	26	05	3	CLN	J3EU			Fishing trawlers of Sri Lanka	
ARSI	7074	0230	22	05	3	CLN	J3EU			Fishing trawlers of Sri Lanka	
ARSI	7090	0233	22	05	3	CLN	J3EU			Fishing trawlers of Sri Lanka	
ARSI	14096.3	0220	13	05	3	CLN	J3EU			Fishing trawlers of Sri Lanka	
ARSI	14250	0200	24	05	3	INS	J3EU			Two OM in QSO, non amateurs.	
ARSI	18160	0130	12	05	3	CHN	A3E			CRI IN CHINESE, STRONG B/C	

CLUB = national radio club or society
kHz = frequency in kHz
UTC = universal time coordinated (GMT)
DD = date (day of month)
MM = month
ITU = ITU-abbreviation (3 letters)
IDENT = ident, call, selcall
MODE = like J3E , A3E, F3E, F1B, G7B
BD = baud
SH = shift
DETAILS = observed details